*********************************************************** 
*                                                           
*  Axalto e-gate USB smart card drivers
*	  version 3.0.6.0
*
*  Installation Readme                                                           
*
************************************************************


************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1.  Overview
2.  System Requirements
3.  Contents of the Distribution Package
4.  List of Available Command Line Flag Options 
5.  List of Available Return Codes 



************************************************************
* 1.  OVERVIEW
************************************************************
The installation program will install to the target system 
the Axalto e-gate USB smart card device drivers.

If a previous version of these drivers is already installed,
the installer will update these drivers to the current version.

The default installation directory is :
	<PROGRAM FILES>\Axalto\e-gate drivers 3.0.6.0



************************************************************
* 2.  SYSTEM REQUIREMENTS 
************************************************************
This software is intended for the following Operating systems :
	Windows 98, Windows 98SE
	Windows Millennium



************************************************************
* 3.  CONTENTS OF THE DISTRIBUTION PACKAGE
************************************************************
The e-gate USB smart card drivers installation package 
contains the following items:

    File(s)       
    -------
    EGATE-9X-SETUP.EXE
    README.TXT (this file)



************************************************************
* 4.  LIST OF AVAILABLE COMMAND LINE FLAG OPTIONS
************************************************************
The installation program supports some command line flags 
for installation options. 

Flag            	Description
----            	-----------
/S              	Silent installation
			A silent installer is an installer which requires
			no user intervention and have no user interface. 

/D=<Install Path>	Overrides the default installation directory



************************************************************
* 5.  LIST OF AVAILABLE RETURN CODES
************************************************************
When the installation completes, the installation program returns
a return code which is one of the following :

  0       		Normal execution (no error)                  
  1       		Installation aborted by user
  2       		The current platform is not supported        
  3       		Administration privileges are required       
  4       		For more information, see log file           
  5       		Unsupported error, see log file              
  10 to 15      	A system restart is required		

When a sytem restart is required to complete the installation process,
the return code is increased by 10.

In addition, a logging file named "egateinstall.log" is created in the
installation directory.

